

|  |  |  |
| --- | --- | --- |
| **Change Note** | | **CN-054** |
| **Change to:** Technical Assumption 70 | | |
| **Description:** Marking of HIU | | |
| **References:** Test regime paragraph 3.7, Submitted documentation | | |
| **Change originator:** FV | | **Date of request:** 30/06/21 |
| **Rev:** 01 | **Date authored:** 12/11/21 | **Proposed change to assumption:** N |

1. Proposed Approach

The unit itself shall be marked with its model name, type number and serial number.

Criteria as previously.

1. Rationale (underlying basis for the change)

Ensures that HIU model, type and serial number are easily identifiable and logged.

1. Impact of change (e.g. implications for test rig)

N/A

|  |  |  |  |
| --- | --- | --- | --- |
| **Evaluation of change** | | | |
| **Date evaluated:** 30/06/21 | **Those present:** GJ, RH, SC, MO & FV | **Additional info required?:** N | **Modification to proposed approach?:** N |
| **Details:** Confirmation of HIU marking | | | |
| **Signed off: Yes** | | | |