

|  |  |  |
| --- | --- | --- |
| **Change Note** | | **CN-046** |
| **Change to:** Technical Assumption47 | | |
| **Description:** HIU orientation | | |
| **References:** Test regime paragraph 2.6, all Tests | | |
| **Change originator:** FV | | **Date of request:** 30/06/21 |
| **Rev:** 01 | **Date authored:** 21/09/21 | **Proposed change to assumption:** N |

1. Proposed Approach

HIU to be oriented vertically.

Criteria as previously.

1. Rationale (underlying basis for the change)

To represent orientation of HIUs when installed.

1. Impact of change (e.g. implications for test rig)

N/A

|  |  |  |  |
| --- | --- | --- | --- |
| **Evaluation of change** | | | |
| **Date evaluated:** 30/06/21 | **Those present:** GJ, RH, SC, MO & FV | **Additional info required?:** N | **Modification to proposed approach?:** N |
| **Details:** Confirmation of HIU orientation | | | |
| **Signed off: Yes** | | | |